### Title: (Title of the abstract must be in sentence case)

*Author & Co-author(s) Name(s)*

Author Affiliation(s) along with email address of the presenter/main author

**Abstract:**

This study presents an analytical model to understand the dynamic behavior of surface-groundwater interaction in a stream-aquifer system in the presence of a clogging layer. The mathematical model consists of an unconfined aquifer of semi-infinite extent resting on a sloping impervious base and interacting with a stream of varying water level. The hydro-interaction is mediated by a thin clogging layer whose hydrologic properties are different from that of the aquifer. The unsteady groundwater flow is approximated by linearized advection-diffusion equation subjected to mixed boundary conditions, including a nonlinear Robin boundary condition. Closed from analytical expressions are developed for water head distribution, flow rate and volumetric exchange of water between stream and aquifer. In few limiting cases, the results reduced to earlier known results. Performance of analytical solution is compared with numerical solution of corresponding nonlinear Boussinesq equation. Sensitivity of the aquifer parameters is analyzed with an illustrative example. (*up to 300 words)*